\begin{center}
\begin{longtable}{lllll}
\caption{\label{tablePhaseRotEb6a}Muon1 component listing of cell \texttt{PhaseRotEb6a}.}
\endfirsthead
\multicolumn{5}{l}{\textbf{continued from previous page}}
\endhead \endfoot \endlastfoot
\hline
RodSource&File&RodAngle&Z\\
\hline
\texttt{TantalumRod}&`pi\_plus\_10GeV.csv'&0.023023&0.22162\\
\hline
Solenoid&Length&Radius&Field\\
\hline
\texttt{S1}&0.42698&0.1&20\\
\texttt{S2}&0.67437&0.2994&4.57958\\
\texttt{S3}&0.31211&0.33213&3.37838\\
\texttt{S4}&0.46206&0.28288&3.46847\\
\texttt{S5}&0.2007&0.27688&1.26126\\
\texttt{S6}&0.66386&0.31742&-2.55856\\
\texttt{S7}&0.46416&0.26787&-2.7027\\
\texttt{S8}&0.75846&0.26156&2.58258\\
\texttt{S9}&0.52372&0.25586&4\\
\texttt{SB1}&0.78298&0.20811&-3.44745\\
\texttt{SB2}&0.78999&0.20751&-3.5035\\
\texttt{SB3}&0.78789&0.20721&-3.52753\\
\texttt{SB4}&0.77598&0.20541&-3.55155\\
\texttt{SB5}&0.77808&0.21141&-3.55956\\
\texttt{SB6}&0.79419&0.2045&-3.52753\\
\texttt{PS1}&0.62883&0.15&3.8959\\
\texttt{PS2}&0.62953&0.15&3.98398\\
\texttt{PS3}&0.64074&0.15&3.95996\\
\texttt{PS4}&0.63584&0.15&4\\
\texttt{PS5}&0.63724&0.15&4\\
\texttt{PS6}&0.63724&0.15&3.99199\\
\hline
Drift&Length&Bore\\
\hline
\texttt{D1}&0.5&0.5\\
\texttt{D2}&0.67017&0.5\\
\texttt{D3}&0.5&0.5\\
\texttt{D4}&0.5005&0.5\\
\texttt{D5}&0.52252&0.5\\
\texttt{D6}&0.5&0.5\\
\texttt{D7}&0.5&0.5\\
\texttt{D8}&0.52653&0.5\\
\texttt{D9}&0.59309&0.5\\
\texttt{DB1}&0.5&0.5\\
\texttt{DB2}&0.5&0.5\\
\texttt{DB3}&0.50501&0.5\\
\texttt{DB4}&0.501&0.5\\
\texttt{DB5}&0.5&0.5\\
\texttt{DB6}&0.5&0.5\\
\texttt{PD1a}&0.33333&0.15\\
\texttt{PD1b}&0.16667&0.15\\
\texttt{PD2a}&0.33367&0.15\\
\texttt{PD2b}&0.16683&0.15\\
\texttt{PD3a}&0.33333&0.15\\
\texttt{PD3b}&0.16667&0.15\\
\texttt{PD4a}&0.33567&0.15\\
\texttt{PD4b}&0.16783&0.15\\
\texttt{PD5a}&0.33333&0.15\\
\texttt{PD5b}&0.16667&0.15\\
\texttt{PD6a}&0.33333&0.15\\
\texttt{PD6b}&0.16667&0.15\\
\hline
RF&Frequency&Radius&Voltage&Phase\\
\hline
\texttt{PRF1}&31.4285\,MHz&0.15&1.68525\,MV&-143.604$^\circ$\\
\texttt{PRF2}&31.4285\,MHz&0.15&1.79067\,MV&-141.802$^\circ$\\
\texttt{PRF3}&31.4285\,MHz&0.15&1.72139\,MV&-130.631$^\circ$\\
\texttt{PRF4}&31.4285\,MHz&0.15&1.72294\,MV&-111.171$^\circ$\\
\texttt{PRF5}&31.4285\,MHz&0.15&1.75452\,MV&-91.7117$^\circ$\\
\texttt{PRF6}&31.4285\,MHz&0.15&1.73074\,MV&-81.6216$^\circ$\\
\hline
\hline
\multicolumn{5}{p{15cm}}{Beamline order: \texttt{TantalumRod}, \texttt{S1}, \texttt{D1}, \texttt{S2}, \texttt{D2}, \texttt{S3}, \texttt{D3}, \texttt{S4}, \texttt{D4}, \texttt{S5}, \texttt{D5}, \texttt{S6}, \texttt{D6}, \texttt{S7}, \texttt{D7}, \texttt{S8}, \texttt{D8}, \texttt{S9}, \texttt{D9}, 3*(\texttt{SB1}, \texttt{DB1}), 3*(\texttt{SB2}, \texttt{DB2}), 2*(\texttt{SB3}, \texttt{DB3}), 3*(\texttt{SB4}, \texttt{DB4}), 3*(\texttt{SB5}, \texttt{DB5}), \texttt{SB6}, \texttt{DB6}, \texttt{SB6}, 7*(\texttt{PD1a}, \texttt{PRF1}, \texttt{PD1b}, \texttt{PS1}), 7*(\texttt{PD2a}, \texttt{PRF2}, \texttt{PD2b}, \texttt{PS2}), 7*(\texttt{PD3a}, \texttt{PRF3}, \texttt{PD3b}, \texttt{PS3}), 7*(\texttt{PD4a}, \texttt{PRF4}, \texttt{PD4b}, \texttt{PS4}), 7*(\texttt{PD5a}, \texttt{PRF5}, \texttt{PD5b}, \texttt{PS5}), 6*(\texttt{PD6a}, \texttt{PRF6}, \texttt{PD6b}, \texttt{PS6})}\\
\hline
\end{longtable}
\end{center}
