\begin{center}
\begin{longtable}{lllll}
\caption{\label{tablePhaseRotLinac1}Muon1 component listing of cell \texttt{PhaseRotLinac1}.}
\endfirsthead
\multicolumn{5}{l}{\textbf{continued from previous page}}
\endhead \endfoot \endlastfoot
\hline
RodSource&File&RodAngle&Z\\
\hline
\texttt{TantalumRod}&`pi\_plus\_10GeV.csv'&0.02002&0.12928\\
\hline
Solenoid&Length&Radius&Field\\
\hline
\texttt{S1}&0.43749&0.1&20\\
\texttt{S2}&0.72903&0.23904&4.92993\\
\texttt{S3}&0.39059&0.27297&-5\\
\texttt{S4}&0.7956&0.34414&-1.48649\\
\texttt{S5}&0.72482&0.3997&3.55155\\
\texttt{S6}&0.85375&0.37357&1.66967\\
\texttt{S7}&0.48238&0.26426&-3.65566\\
\texttt{S8}&0.88108&0.3997&-2.75876\\
\texttt{S9}&0.7017&0.25255&-4\\
\texttt{SB1}&0.86496&0.1979&-4\\
\texttt{PS1}&0.8993&0.15&4\\
\texttt{LS1}&0.9&0.15&-4\\
\hline
Drift&Length&Bore\\
\hline
\texttt{D1}&0.5&0.5\\
\texttt{D2}&0.55455&0.5\\
\texttt{D3}&0.7973&0.5\\
\texttt{D4}&0.5&0.5\\
\texttt{D5}&0.89139&0.5\\
\texttt{D6}&0.9985&0.5\\
\texttt{D7}&0.5&0.5\\
\texttt{D8}&0.91041&0.5\\
\texttt{D9}&0.83884&0.5\\
\texttt{DB1}&0.5&0.5\\
\texttt{PD1a}&0.33333&0.15\\
\texttt{PD1b}&0.16667&0.15\\
\texttt{LD1a}&0.33333&0.15\\
\texttt{LD1b}&0.16667&0.15\\
\hline
RF&Frequency&Radius&Voltage&Phase\\
\hline
\texttt{PRF1}&31.4285\,MHz&0.15&2.24887\,MV&41.6216$^\circ$\\
\texttt{RF1}&88\,MHz&0.15&0\,MV&156.577$^\circ$\\
\hline
\hline
\multicolumn{5}{p{15cm}}{Beamline order: \texttt{TantalumRod}, \texttt{S1}, \texttt{D1}, \texttt{S2}, \texttt{D2}, \texttt{S3}, \texttt{D3}, \texttt{S4}, \texttt{D4}, \texttt{S5}, \texttt{D5}, \texttt{S6}, \texttt{D6}, \texttt{S7}, \texttt{D7}, \texttt{S8}, \texttt{D8}, \texttt{S9}, \texttt{D9}, 29*(\texttt{SB1}, \texttt{DB1}), \texttt{SB1}, 60*(\texttt{PD1a}, \texttt{PRF1}, \texttt{PD1b}, \texttt{PS1}), 60*(\texttt{LD1a}, \texttt{RF1}, \texttt{LD1b}, \texttt{LS1})}\\
\hline
\end{longtable}
\end{center}
